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ROpigi nomazgdjiet rokas
Tad higiéniski nozaveéjiet
rokas ar gaisu, kas atfirits
ar HEPA filtru

Visi Dyson Airblade™ roku Zavétaiji
aprikoti ar HEPA filtru. ' Ta gaiss
tualetes istaba tiek atfirits pirms
JUs saksiet Zavét rokas.
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Zavé rokas ar gaisu, kas atfirits ar

HEPA filtru. Zavégana ar firu gaisu.

Visi Dyson Airblade™ roku zavétaji aprikoti
ar HEPA filtru. ' Ta gaiss tualetes istaba tiek
aftfirits pirms JUs saksiet zavét rokas.
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Zavé rokas ar gaisu, kas atfirits ar

HEPA filtru. Zavé$ana ar firu gaisu.

Visi Dyson Airblade™ roku zavetaji aprikoti
ar HEPA filtiru. ' Ta gaiss tualetes istaba tiek
attirits pirms JUs saksiet zavét rokas.

'HEPA filtrs testéts neatkarigaja laboratorija saskana ar
EN 1822-5 standarta noteikumiem un nosacijumiem.
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To insert a logo into the backboard
please follow these instructions

In MS word go to: ‘Insert pictures’ > ‘Pictures’ >
‘Picture from file’ > then choose the logo to be inserted.
Click ‘Insert.” The logo should appear on the backboard.

Select the logo and then go to:
‘Text wrap’ and select ‘In front of text.’
You can then place the logo in correct position.










