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dyson airblade

ROpigi nomazgdjiet rokas
Tad higiéniski nozaveéjiet
rokas ar gaisu, kas atfirits
ar HEPA filtru

Visi Dyson Airblade™ roku Zavétaiji
aprikoti ar HEPA filtru. ' Ta gaiss
tualetes istaba tiek atfirits pirms
JUs saksiet Zavét rokas.
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Zavé rokas ar gaisu, kas atfirits ar

HEPA filtru. Zavégana ar firu gaisu.

Visi Dyson Airblade™ roku zavétaji aprikoti
ar HEPA filtru. ' Ta gaiss tualetes istaba tiek
aftfirits pirms JUs saksiet zavét rokas.
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Žāvē rokas ar gaisu, kas  
attīrīts ar HEPA filtru.  
Žāvēšana ar tīru gaisu.   
Visi Dyson Airblade™  
roku žāvētāji aprīkoti  
ar HEPA filtru. 1  
Tā gaiss tualetes istabā  
tiek attīrīts pirms Jūs  
sāksiet žāvēt rokas.



1�HEPA filtrs testēts neatkarīgajā laboratorijā saskaņā ar  
EN 1822-5 standarta noteikumiem un nosacījumiem.
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To insert a logo into the backboard  
please follow these instructions



In MS word go to: ‘Insert pictures’ > ‘Pictures’ > 
‘Picture from file’ > then choose the logo to be inserted.
Click ‘Insert.’ The logo should appear on the backboard.



Select the logo and then go to:  
‘Text wrap’ and select ‘In front of text.’
You can then place the logo in correct position.
   











